|  |  |
| --- | --- |
| **Aecon Business:** | Major Projects East |
| **Project / Location:** | BNA (Gordie Howe) Canadian Bridge Pier 14 |

|  |  |
| --- | --- |
| **Associated Serious Event Flash:** | Lost Time (mild to severe concussion requiring 4 days away from work) |

|  |
| --- |
| **Event Summary:** |
| |  | | --- | |  |  |  | | --- | | The incident occurred at the BNA (Gordie Howe) Canadian Bridge Pier 14 project site on October 16th, 2024. An electric 2-inch water pump weighing 26lbs fell 18’4” and struck a laborer on the back of the hard hat. The laborer had just descended the ladder to the bottom of the pier tower when the pump hit him. The worker was assigned the task of pumping water out of the pier leg from the inside.  The worker did not lose consciousness and remained on his feet. His tool belt hung on the power cord at the top of the ladder and when he reached the bottom, he inadvertently pulled the pump from the concrete platform 18' 4" above him. The pump was behind a horizontal scaffold tube which was 5 ¾ inches in height. The hard hat involved in the incident was not a BNA issued hard hat but met the code requirements specified in the BNA Safety Plan.  The immediate outcome was that operations were stopped and the scene was frozen for an initial investigation. This resulted in schedule and production delays. The worker was taken to an offsite medical clinic and was diagnosed with a mild to severe concussion and placed off work until Oct 23, 2004, due to standard concussion protocols. The broader impacts included potential severe/fatal injuries due to drop object, project shutdown, loss of production, fines, and legislative consequences, and jeopardizing our reputation and integrity with the trades, unions, and legislative authorities.  Contributing Factors:  - Equipment tethers were not being utilized at the time of the accident. - The water pump was not adequately secured or fastened on the platform pier. - False sense of security that the horizontal tube rail was adequate prevention for dropped objects. - A two-inch pump was used to remove the bulk of the water but never hoisted out of the pier once it was not required. - The pump was relocated to the concrete platform in the center of the pier and a “puddle pump” was put in place to remove the remainder of the water. - The power cord of the two-inch pump is approximately 2 foot short of the bottom of the pier providing additional tension to the cord. | |

|  |
| --- |
| **Lessons Learned to Share** |
| - Ensure all equipment is properly secured or fastened to prevent potential drop object hazards. - Do not rely solely on physical barriers for dropped object prevention. - Regularly complete verifications for BNA’s “Safety Absolutes” equivalent to Aecon’s Fatal 8 activity for WAH (PUE- Dropped Object) for compliance. - Immediately remove unnecessary tools and equipment that are not needed inside the pier towers. - Follow and verify all dropped object prevention SOP’s and requirements developed for BNA project. |

|  |  |  |
| --- | --- | --- |
| **Contact for Further Information** | **Name:** | **Email Address:** |

Pictures on The Next Page

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |
|  |  |  |

|  |  |  |
| --- | --- | --- |
| **Supporting Picture** |  | **Supporting Picture** |
|  |  |