|  |  |
| --- | --- |
| **Aecon Business:** | Major Projects East |
| **Project / Location:** | BNA (Gordie Howe) Canadian Bridge Pier 14 |

|  |  |
| --- | --- |
| **Associated Serious Event Flash:** | Lost Time (mild to severe concussion requiring 4 days away from work) |

|  |
| --- |
| **Event Summary:** |
| |  | | --- | |  |  |  | | --- | | On October 16th, 2024, a serious incident occurred at the BNA (Gordie Howe) Canadian Bridge Pier 14, managed by Aecon's Major Projects East sector. An electric 2-inch water pump, weighing 26lbs, fell from a height of 18'4", striking a laborer on the back of his hard hat. The laborer had just descended the ladder to the bottom of the pier tower when the pump fell on him. The worker was assigned the task of pumping water out of the pier leg from the inside.  The worker did not lose consciousness and remained on his feet. His tool belt hung on the power cord at the top of the ladder, and when he reached the bottom, he inadvertently pulled the pump from the concrete platform above him. The pump was located behind a horizontal scaffold tube, which was 5 ¾ inches in height. The hard hat involved in the incident was not a BNA issued hard hat but met the code requirements specified in the BNA Safety Plan.  The immediate outcome of the incident was a halt in operations for an initial investigation, causing schedule and production delays. The worker was sent to an offsite clinic due to the damage noted on the hard hat, the weight of the pump, the distance of the drop, and the energy created. He was diagnosed with a mild to severe concussion and was off work until October 23, 2024. The potential impacts of the incident included severe or fatal injuries, project shutdown, loss of production, fines, legislative consequences, and damage to our reputation and integrity with the trades, unions, and legislative authorities.  Contributing Factors:  - Lack of equipment tethers at the time of the accident - Inadequate securing of the water pump on the platform pier - False sense of security provided by the horizontal tube rail - Presence of additional clutter and tools in a tight work location - Inadequate length of the power cord of the two-inch pump - Inadvertent pulling of the pump by the worker | |

|  |
| --- |
| **Lessons Learned to Share** |
| - Need for a "Process Flow" to prevent dropped objects - Regular completion of verifications for BNA’s “Safety Absolutes” - Requirement for BNA craft to wear JV provided hard hat and Aecon staff to wear approved class e, type 2 hard hats with chin straps - Importance of visual assessment of tasks to prevent entanglement with surrounding objects and cords - Immediate removal of unnecessary tools and equipment from the pier towers - Strict adherence to all dropped object prevention SOP’s and requirements developed for BNA project. |

|  |  |  |
| --- | --- | --- |
| **Contact for Further Information** | **Name:** | **Email Address:** |

Pictures on The Next Page

|  |  |  |
| --- | --- | --- |
| **Supporting Picture** |  | **Supporting Picture** |
|  |  |

|  |  |  |
| --- | --- | --- |
| **Supporting Picture** |  | **Supporting Picture** |
|  |  |