|  |  |
| --- | --- |
| **Aecon Business:** | Major Projects East |
| **Project / Location:** | BNA (Gordie Howe) Canadian Bridge Pier 14 |

|  |  |
| --- | --- |
| **Associated Serious Event Flash:** | Lost Time (mild to severe concussion requiring 4 days away from work) |

|  |
| --- |
| **Event Summary:** |
| |  | | --- | |  |  |  | | --- | | Event Summary:  An electric 2-inch water pump fell 18’4” striking a laborer on the back of the hard hat. The laborer had just descended the ladder to the bottom of the pier tower when the pump struck him on the back of the hard hat. The injured worker did not lose consciousness and remained on his feet.  Contributing Factors:  - - Equipment tethers not being utilized  - - Water pump not adequately secured  - - False sense of security with existing safety measures  - - Clutter and tools in work location  - - Power cord tension causing pump to tip over | |

|  |
| --- |
| **Lessons Learned to Share** |
| Lessons Learned:  - - Implement process flow to prevent dropped objects  - - Regular verifications for safety compliance  - - Increased drop object blitzes  - - Wear approved hard hats with chin straps  - - Visually assess tasks to prevent entanglement  - - Remove unnecessary tools and equipment immediately  - - Follow and verify all dropped object prevention SOP’s and requirements |

|  |  |  |
| --- | --- | --- |
| **Contact for Further Information** | **Name:** | **Email Address:** |

Pictures on The Next Page

|  |  |  |
| --- | --- | --- |
| **Supporting Picture** |  | **Supporting Picture** |
|  | Supporting Pictures: |

|  |  |  |
| --- | --- | --- |
| **Supporting Picture** |  | **Supporting Picture** |
|  |  |

## Supporting Pictures

|  |  |
| --- | --- |
|  |  |
|  |  |
| [Image failed] |  |
|  |  |
|  |  |
|  |  |