|  |  |
| --- | --- |
| **Aecon Business:** | Major Projects East |
| **Project / Location:** | BNA (Gordie Howe) Canadian Bridge Pier 14 |

|  |  |
| --- | --- |
| **Associated Serious Event Flash:** | Lost Time (mild to severe concussion requiring 4 days away from work) |

|  |
| --- |
| **Event Summary:** |
| |  | | --- | |  |  |  | | --- | | **Worker struck by falling water pump.**  A laborer was struck on the back of the hard hat by a falling 2-inch electric water pump, weighing 26lbs, from a height of 18’4”. The worker had just descended a ladder inside the pier tower when the pump fell. The pump was being used to remove water from the pier leg. The worker remained conscious and on his feet after the incident. His tool belt had become entangled with the pump's power cord, causing the pump to be pulled from its platform when the worker reached the bottom of the ladder. Operations were halted for an initial investigation, causing schedule and production delays. The worker was sent to an offsite clinic and diagnosed with a mild to severe concussion, requiring time off work until Oct 23, 2024.  The following key **contributing factors** were identified:  - The water pump was not secured or fastened to prevent it from falling. - Equipment tethers were not being used because they were thought to be unnecessary. - The pump was placed behind a horizontal scaffold tube, creating a false sense of security. - The pump was not removed from the pier once it was no longer needed, adding clutter to the work area. - The power cord of the pump was short, adding tension and contributing to the pump being pulled off the platform. | |

|  |
| --- |
| **Lessons Learned to Share** |
| - Implement a process to prevent dropped objects, such as securing or fastening objects, or installing physical barricades or mesh curtains. - Regularly complete verifications for safety compliance. - Ensure workers wear approved hard hats with chin straps. - Assess tasks visually to prevent entanglement with surrounding objects and cords. - Remove unnecessary tools and equipment from work areas promptly. - Follow and verify all dropped object prevention SOP’s and requirements. |

|  |  |  |
| --- | --- | --- |
| **Contact for Further Information** | **Name:** | **Email Address:** |

Pictures on The Next Page

|  |  |  |
| --- | --- | --- |
| **Supporting Picture** |  | **Supporting Picture** |
|  |  |

|  |  |  |
| --- | --- | --- |
| **Supporting Picture** |  | **Supporting Picture** |
|  |  |